

**BvNET Driver Installation Guide Windows XP or higher**

## Driver Installation on Windows XP or higher

Please proceed with the following steps to install the driver:

1. Please locate the BvNet Drivers Folder either on the CD-ROM or where you have copied the drivers to if you downloaded them. **Do not plug in your BvNet USB device until the installation has completed**.
2. Run “BvNet Driver Installation”. This will run the BvNet driver installation program. Two drivers will be pre-installed.
3. You can now plug in your BvNet device. Upon first connection, Windows will locate the drivers and a message should appear on your taskbar informing you that the drivers have been installed successfully. Your BvNet device is now ready to use.
4. An entry will be added to Windows Control Panel (Programs and Features) if you wish to uninstall the drivers.

## Driver installation on Windows 2000

This version of the driver does not support Windows 2000. Please download BvNET USB Driver V2.06.00 from the Linea Research website.